> Back to Contents Page

> ## Specifications: Broadcom NetXtreme® 57XX User Guide

> 10/100/1000BASE-T Cable Specifications

> Performance Specifications

> Physical Characteristics

> Power Requirements

> Environmental Specifications

> ### 10/100/1000BASE-T Cable Specifications

> Table 1. 10/100/1000BASE-T Cable Specifications
> Port Type | Connector | Media | Maximum Distance
> --- | --- | --- | ---
> 10BASE-T | RJ-45 | Category 3, 4, or 5 unshielded twisted pairs (UTP) | 100m (328 ft)
> 100/1000BASE-T1 | RJ-45 | Category 52 UTP | 100m (328 ft)
> 11000BASE-T signaling requires 4 twisted pairs of Category 5 balanced cabling, as specified in ISO/IEC 11801:1995 and ANSI/EIA/TIA-568-A (1995) and tested for additional performance using testing procedures defined in TIA/EIA TSB95. 2Category 5 is the minimum requirement. Category 5e and Category 6 are fully supported.

> ### Performance Specifications

> Table 2. Performance Specifications
> Feature | Specification
> --- | ---
> PCI Type Controllers (Single-Port BCM570X Controllers)
> PCI Clock | 66 MHz maximum
> PCI-X Clock | 133 MHz
> PCI/PCI-X Data/Address | 32-bit and 64-bit
> PCI-X Data Burst Transfer Rate | 400 Mbit/s (32-bit bus at 100 MHz) 800 Mbit/s (64-bit bus at 100 MHz) 600 Mbit/s (32-bit bus at 100 MHz) - BCM5701/BCM5703 only 1024 Mbit/s (64-bit bus at 100 MHz) - BCM5701/BCM5703 only
> PCI Data Burst Transfer Rate | 132 Mbit/s (32-bit bus) 264 Mbit/s (64-bit bus) 528 Mbit/s (64-bit bus at 66 MHz)
> PCI Modes | Master/slave
> PCI Express™ Type Controllers (BCM57XX Controllers)
> PCI Express Interface | x1 link width
> PCI Express Aggregated Bandwidth (transmit and receive) | 2.5 Gbps
> 10/100/1000BASE-T | 10/100/1000 Mbps (full-duplex)

> ### Physical Characteristics

> Table 3. Physical Characteristics
> NIC Type | Length | Width
> --- | --- | ---
> PCI | 16.6 cm (6.6 in.) | 6.45 cm (2.54 in.)
> PCI Express | 11.2 cm (4.420 in.) | 5.08 cm (2.00 in.)

> ### Power Requirements

> Table 4. Power Requirements
> Item | Value
> --- | ---
> BCM5700 and BCM5701
> Operating Voltage | +5V ± 5%
> Power Consumption | 10W 2A @ +5VDC
> BCM5703
> Operating Voltage | +3.3V ±10% for BCM95703A30 and BCM95703SA31 +5V ±5% for BCM95703A30U and BCM95703SA31U
> Power Consumption | 4W 1.2A@ +3.3V for BCM95703A30
> BCM5721 and BCM5751
> Operating voltage | +3.3V ± 10%
> Power Consumption | 2.84W 860 mA @ +3.3VDC
> BCM5705
> Operating Voltage | +3.3V ± 10%
> Power Consumption | 1.13W maximum

> ### Environmental Specifications

> Table 5. Environmental Specifications
> Condition | Operating Specification | Storage Specification
> --- | --- | ---
> Temperature | 0°C to 55°C (+32°F to +131°F) | –40°C to +85°C (–40°F to +185°F)
> Relative Humidity | 5% to 85% (non-condensing) 40°C, 16-hour dwells at extremes | 5% to 95% (non-condensing) 10°C/hour
> Altitude | Up to 10,000 ft. | Up to 35,000 ft.
> Shock | 10g, 1/2 sine wave, 11 ms | 60g, 1/2 sine wave, 11 ms
> Vibration, peak-to-peak displacement | 0.005 in. max (5 Hz to 32 Hz) | 0.1 in. max (5 Hz to 17 Hz)
> Vibration, peak acceleration | 0.25g (5 Hz to 500 Hz) (Sweep Rate = 1 octave/min.) | 0.25g (5 Hz to 500 Hz) (Sweep Rate = 1 octave/min.)

> Back to Contents Page